|  |  |  |  |
| --- | --- | --- | --- |
| Name and surname: |  | Title |  |
| Date of birth |  | | |
| Employer |  | | |

The following minimum requirements for vision ability according to EN ISO 9712 are certified:

**1. Near vision:**

Near vision acuity shall permit reading of at minimum Jaeger test no. 1 or Times New Roman 4,5 or equivalent letters (having height of 1,6 mm) at distance not less than 30 cm with one or both eyes, either corrected or uncorrected

or

Near vision according to EN ISO 18490

without correction

with correction

**2. Sufficient colour distinguishability (e.g. according to Ishiara)**

Sufficient distinguishability of colours or shades of grey, which are used in NDT methods/ techniques, as specified by the employer.

The applicant is able

The applicant is not able

Near vision acuity testing, colour vision and/or grey scale perception verification(s) shall be administered by a licensed physician, nurse, ophthalmologist or optometrist; or by another trained professional who is approved and documented by a Level 3 personnel acting on behalf of the employer.

|  |  |  |
| --- | --- | --- |
|  |  |  |
| Place | Date | Stamp and signature of the examining person |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| Place | Date | Stamp and signature of employer representative |