|  |  |  |  |
| --- | --- | --- | --- |
| Name and surname: |       | Title |       |
| Date of birth |       |
| Employer |       |

The following minimum requirements for vision ability according to EN ISO 9712 are certified:

**1. Near vision:**

Near vision acuity shall permit reading of at minimum Jaeger test no. 1 or Times New Roman 4,5 or equivalent letters (having height of 1,6 mm) at distance not less than 30 cm with one or both eyes, either corrected or uncorrected

or

[ ]  Near vision according to EN ISO 18490

[ ]  without correction

[ ]  with correction

**2. Sufficient colour distinguishability (e.g. according to Ishiara)**

Sufficient distinguishability of colours or shades of grey, which are used in NDT methods/ techniques, as specified by the employer.

[ ]  The applicant is able

[ ]  The applicant is not able

Near vision acuity testing, colour vision and/or grey scale perception verification(s) shall be administered by a licensed physician, nurse, ophthalmologist or optometrist; or by another trained professional who is approved and documented by a Level 3 personnel acting on behalf of the employer.

|  |  |  |
| --- | --- | --- |
|  |  |  |
| Place | Date | Stamp and signature of the examining person |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| Place | Date | Stamp and signature of employer representative |