|  |  |  |  |
| --- | --- | --- | --- |
| Name and surname: |  | Title |  |
| Date of birth |  | | |
| Employer |  | | |

The following minimum requirements for vision ability according to EN ISO 9712 are certified:

**1. Near vision:**

Near vision acuity shall permit reading of at minimum Jaeger test no. 1 or Times New Roman 4,5 or equivalent letters (having height of 1,6 mm) at distance not less than 30 cm with one or both eyes, either corrected or uncorrected.

without correction

with correction

**2. Sufficient colour distinguishability (e.g. according to Ishiara)**

Sufficient distinguishability of colours or shades of grey, which are used in NDT methods/ techniques, as specified by the employer.

The applicant is able

The applicant is not able

|  |  |  |
| --- | --- | --- |
|  |  |  |
| Place | Date | Stamp and signature  of ophthalmologist or optician |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| Place | Date | Stamp and signature of employer representative |